Exit doors

Are doors required to serve as exits designed and constructed so that the way of exit travel is obvious and direct?

Are windows that could be mistaken for exit doors made inaccessible by barriers or railing?

Are exit doors able to open from the direction of exit travel without the use of a key or special knowledge or effort?

Is a revolving, sliding, or overhead door prohibited from serving as a required exit door?

When panic hardware is installed on a required exit door, will it allow the door to open by applying a force of 15 pounds or less in the direction of the exit traffic?

Are doors on cold-storage rooms provided with inside release mechanisms that release the latches and open the doors even they are padlocked or otherwise locked on the outside?

Where exit doors open directly onto a street, alley, or other area where vehicles may be operated, are adequate barriers and warnings provided to prevent employees from stepping directly into traffic?

Do doors that swing both directions have viewing panels in each door if they are frequently used?