Exits

Are all exits marked with an exit sign and illuminated by a reliable light source if used in darkness?

Are directions to exits marked with visible signs if the exits are not immediately apparent?

Are doors, passageways, or stairways that are neither exits nor access to exits, and that could be mistaken for exits, marked “NOT AN EXIT,” or “TO BASEMENT,” “STOREROOM,” and the like?

Are exit signs provided with the word “EXIT” in lettering at least six inches high and the stroke of the lettering at least 3⁄4-inch wide?

Are exit doors side-hinged?

Are all exits kept free of obstructions and unlocked?

Are at least two means of egress provided from elevated platforms, pits, or rooms where the absence of a second exit would increase the risk of injury from hot, poisonous, corrosive, suffocating, flammable, or explosive substances?

Are there sufficient exits to permit prompt escape in emergencies?

Are the number of exits from each floor of a building and the number of exits from the building itself appropriate for the building occupancy load?

When workers must exit through glass doors, storm doors, and such are the doors fully tempered and do they meet safety requirements for human impact?