Floor and wall openings

Are floor holes or openings guarded by a cover, guardrail, or equivalent on all sides (except at entrance to stairways or ladders)?

Are toe-boards installed around the edges of a permanent floor opening (where persons may pass below the opening)?

Are skylight screens constructed and mounted to withstand a load of at least 200 pounds?

Is the glass in windows, doors, and glass walls which may be subject to human impact appropriate for its use?

Are grates or similar covers over floor openings such as floor drains designed so that the grate spacing will not catch foot traffic or rolling equipment?

Are unused service pits and portions of such pits covered or protected by guardrails or the equivalent?