Personal protective equipment (PPE)

Have you assessed workplace hazards that might require PPE and reviewed related injuries?

Has the assessment been documented?

Does the documentation identify the workplace evaluated?

Has training been provided to each employee who is required to wear PPE?

Has the training been documented?

Are protective goggles or face shields provided to employees and worn when there may be danger of flying material or caustic or corrosive materials?

Are ANSI-approved safety glasses worn at all times in areas where there is risk of eye injury?

Are protective gloves, aprons, or shields provided to employees for protection against cuts, corrosive liquids, and chemicals?

Are hardhats provided and worn where there is a danger of falling objects?

Are hardhats inspected periodically for damage to the shell and the suspension system?

Do employees exposed to vehicular traffic wear high visibility garments that make them stand out from their surroundings?

Do workers wear reflective garments at night?

Are appropriate respirators provided for regular or emergency use where they are necessary?

Is there a written respirator program?

Are the respirators inspected before and after each use?

Is a written record kept of all inspection dates and findings?

Have all employees been trained in work procedures, and proper use and maintenance of protective clothing and equipment for cleaning up spilled toxic or other hazardous materials or liquids?

Is a spill kit available for employees to clean up spilled toxic or hazardous materials?

Are employees required to wear safety shoes when they are exposed to conditions that could cause foot injuries?

Is all protective equipment sanitary and ready to use?

Is there an eyewash facility and a quick-drench shower in each work area where employees are exposed to caustic or corrosive materials?

Do employees have lunch areas in areas where there is no exposure to toxic materials?

Is protection from occupational noise provided when sound levels exceed those of the OR-OSHA hearing conservation standard — 1910.95?