Walkways

Are aisles and passageways kept clear and at least 22 inches wide?

Are aisles and walkways appropriately marked?

Are wet surfaces covered with non-slip materials?

Are openings or holes in the floors or other walking surfaces repaired or otherwise made safe?

Is there a safe clearance for walking in aisles in which vehicles operate?

Are materials and equipment stored so sharp objects do not obstruct the walkway?

Are changes of direction or elevation easily identified?

Do aisles or walkways near moving or operating machinery, welding, and similar operations keep employees away from hazards?

Is there floor-to-headroom height of at least 6.5 feet provided for the entire length of any walkway?

Are standard guardrails provided wherever aisle or walkway surfaces are elevated more than four feet above floor or ground?

Are bridges provided over conveyors and similar hazards?