**WORKPLACE AUDIT / INSPECTION REPORT**

**Compressed Gas Storage Area**

**Location: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Audited by:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Audit Item/ Practice**

**Check if item / Practice not in compliance**

**General**

Are cylinders legibly marked to identify the gas contained in them?

Are compressed gas cylinders stored in areas away from heat sources?

Are cylinders stored in a manner to prevent them creating a hazard by tipping, falling, or rolling?

Are all valves closed off before a cylinder is moved, when the cylinder is empty, and at the completion of each job?

Are low pressure fuel-gas cylinders checked periodically for corrosion, general distortion, cracks, or any other defect that might indicate a weakness or render it unfit for service?

Does the periodic check of low pressure fuel-gas cylinders include a close inspection of the cylinder's bottom?

If compressed air is used for cleaning off clothing, is the pressure reduced to less than 10 psi?

If welding gases are stored, are oxygen and acetylene separated by a 5 foot non-combustible barrier? .253 (b)(4)

**LP Gas**

Is liquified petroleum gas stored, handled, and used in accordance with safe practices and standards?

Are "NO SMOKING" signs posted on liquified petroleum gas tanks?

Are liquified petroleum storage tanks guarded to prevent damage from vehicles?

Are fuel gas cylinders and oxygen cylinders separated by distance, fire resistant barriers, etc., while in storage?

**Fire Protection**

If you have a fire alarm system, is it tested bimonthly? .165

Are all fire extinguishers accessible, and their locations clearly designated? .157

Are all fire extinguishers inspected and recharged regularly, and noted on the inspection tag? .157

Repairs/corrections must be completed by (date) \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Routed to \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Repairs/corrections from above have been done.

Supervisor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_