Elevated surfaces

Have you posted signs, when appropriate, that show load capacities of elevated floors?

Are elevated surfaces (more than four feet above the floor or ground) provided with standard guardrails?

Are all elevated surfaces beneath which people or machinery could be exposed to falling objects provided with standard toe-boards?

Is a permanent means of access/egress provided to elevated work surfaces?

Is material on elevated surfaces piled, stacked, or racked to prevent it from tipping, falling, collapsing, rolling, or spreading?

Are dock boards or bridge plates used when transferring materials between docks and trucks or railcars?

Are dock boards or bridge plates secured in place when they are in use?